{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["工程量清单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"工程量清单","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"merged":[[0,0,0,7],[1,0,1,7],[22,0,22,6],[23,2,23,5]],"flags":["formulas_cached_only"]}
["嘉兴市级应急物资储备库视频监控系统工程量清单"]
["工程说明：仓库一楼二楼安装视频监控设备，前端12个点位，现场自行勘探。"]
["序号","项目名称","品牌","项目特征","单位","数量","单价（元）","总价（元）"]
[1,"监控摄像设备","海康威视/大华/宇视","名称：网络摄像机\n外形：筒型\n镜头参数：4mm\n分辨率：3200*1800\n供电方式：DC12V、POE\n压缩格式：H.264、H.265、smart265\n补光距离：红外光最远50米\n网络接口：10Base-T/100Base-TX(RJ-45)\n协议支持：NETIP ONVIF\n","个",12]
[2,"支架","海康威视/大华/宇视","名称：监控支架\n材质：铝合金\n安装方式：壁装\n","个",12]
[3,"网络线","康普/一舟/诚讯","名称：超五类网线\n屏蔽类型：非屏蔽\n外套材质：PVC\n线芯材质：无氧铜\n绝缘材料：高密度聚乙烯\n规格线长：305米","箱",3]
[4,"电源线","正泰/缆星国际/诚讯","名称：二芯软护套线\n规格：RVV2*1MM\n导体材质：无氧铜\n绝缘材质：阻燃聚乙烯PC\n额定电压：450V/750V\n规格线长：100米","卷",2]
[5,"PVC管","中财/上丰/井久","名称：PVC线管\n规格：D20\n壁厚：1.2mm\n","米",400]
[6,"接线板","公牛/国际电工/正泰","名称：多用接线板\n额定电压：AC250V\n最大电流：10A\n最大功率：2500W","个",3]
[7,"弱电箱","视明通/正泰/定制","名称：监控设备箱\n材质：不锈钢\n规格：300*400*180 带锁\n","个",2]
[8,"网络机柜","图腾/大唐保镖/定制","名称：网络机柜\n材质：优质冷轧钢、脱脂静电喷漆\n高度：500mm（9U）\n宽度：550mm\n深度：450mm","个",1]
[9,"硬盘录像机","海康威视/大华/宇视","名称：网络硬盘录像机\n网络视频输入：16路\n输入带宽：160Mbps\n解码能力：H.264、H.265、smart265\n输出：hdmi*1、vga*1、video*1\n硬盘接口：SATA*2\n其他接口：RJ45口*1、USB*2\n\n","台",1]
[10,"存储硬盘","海康威视/西部数据/希捷","名称：监控硬盘\n容量：8T\n类型：3.5寸监控级机械硬盘\n接口：SATA","个",1]
[11,"监控交换机","海康威视/TPLINK/MERCURY","名称：监控poe交换机\n端口数量：8口\n上行速率：10/100/1000Mbps\n单口poe功率：15.4W\n外壳：金属\n","台",1]
[12,"监控交换机","海康威视/TPLINK/MERCURY","名称：监控poe交换机\n端口数量：16口\n上行速率：10/100/1000Mbps\n单口poe功率：15.4W\n外壳：金属\n","台",1]
[13,"路由器","海康威视/TPLINK/MERCURY","名称：有线路由器\nWAN接口：10/100/1000Mbps*1\nLAN接口：10/100/1000Mbps*4\n其他：支持上网行为管理、WEB认证、防火墙、带宽控制\n外壳:金属\n","台",1]
[14,"液晶显示屏","长虹/小米/TCL","名称：液晶电视机\n屏幕尺寸：43英寸\n分辨率：1920*1080\n接口：HDMI*1、USB*1、RJ45*1、AV*1","台",1]
[15,"电视机支架","长虹/小米/TCL","名称：电视机支架\n安装方式：壁装 壁挂\n材质：金属","个",1]
[16,"网络跳线","诚讯/康普/一舟","名称：成品网线\n性能等级：超五类\n屏蔽类型：非屏蔽\n外套材质：PVC\n线芯材质：无氧铜\n绝缘材料：高密度聚乙烯\n规格线长：3米\n","根",4]
[17,"高清线","绿联/秋叶原/优越者","名称：HDMI成品视频线\n屏蔽类型：双屏蔽\n外被性能：PVC\n线长：10米","根",1]
[18,"无线鼠标","罗技/雷柏/联想","名称：无线鼠标\n工作方式：光电\n连接方式：2.4G\n","个",1]
[19,"施工辅材","国产","卡钉 卡攀 管材 水晶头 网线等 包工包料","批",1]
["合计"]
[null,null,"报价单位："]